<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-PowerIC-V_REG_TPS76433-SOT23-5">
<!-- generated from Sparkfun Eagle Library 'SparkFun-PowerIC' V_REG_TPS76433 SOT23-5 -->
<version>4</version>
<date>2013-02-13</date>
<label>IC</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;
Older TI part. LDO 150mA regulator. No output by-pass cap option. See V_REG_LDO for a better part.</description>
<title>Voltage Regulator</title>
<tags>
<tag>V_REG_TPS76433</tag>
<tag>SOT23-5</tag>
</tags>
<properties>
<property name="package">sot23-5</property>
<property name="family">sparkfun Voltage Regulator</property>
<property name="chip">TPS76433</property>
<property name="variant">sot23-5</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-poweric_sot23-5_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-poweric_tps76433dbvt_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-poweric_sot23-5_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-poweric_sot23-5_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector2" name="EN" type="male">
<description>EN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="IN" type="male">
<description>IN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="OUT" type="male">
<description>OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>