<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1255" moduleId="1234DBDC00">
 <version replacedby="2244EBEC10">2</version>
 <author>Stefan Hermann</author>
 <title>NPN-Transistor</title>
 <label>Q</label>
 <date>2008-10-10</date>
 <tags>
  <tag>NPN</tag>
  <tag>transistor</tag>
  <tag>signal transistor</tag>
  <tag>aplifier</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="package">TO92 [THT]</property>
  <property name="family">obsolete Bipolar Transistor</property>
  <property name="doping">NPN</property>
 </properties>
 <description>A standard NPN-transistor</description>
 <views>
  <iconView>
   <layers image="icon/basic_transistor_npnicon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/basic_transistor_npn.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView fliphorizontal="true" flipvertical="true">
   <layers image="schematic/basic_transistor_npn.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/to92.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="emitter" type="male">
   <description>emitter</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="base" type="male">
   <description>base</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" name="collector" type="male">
   <description>collector</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>