<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='LilyPad-Button-v12'>
<version>4</version>
<date>2013-05-26</date>
<author>Fabian Althaus</author>
<description>We designed this board to give the user a very discrete button without any sharp edges. Button closes when you push it and opens when you release (momentary push button).

LilyPad is a wearable e-textile technology developed by Leah Buechley and cooperatively designed by Leah and SparkFun. Each LilyPad was creatively designed to have large connecting pads to allow them to be sewn into clothing. Various input, output, power, and sensor boards are available. They&apos;re even washable!

Note: A portion of this sale is given back to Dr. Leah Buechley for continued development and education of e-textiles.

Dimensions:

8x16mm
Thin 0.8mm PCB</description>
<title>LilyPad Button Board</title>
<url>http://www.sparkfun.com/products/8776</url>
<tags>
<tag>Lilypad</tag>
<tag>Button</tag>
</tags>
<properties>
<property name='family'>microcontroller board (lilypad)</property>
<property name='Dimensions'>5.2mm x 5.2mm</property>
<property name='type'>Button</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/LilyPad-Button-v12_breadboard.svg'>
<layer layerId='breadboardbreadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/LilyPad-Button-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/LilyPad-Button-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/LilyPad-Button-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector0' type='female' name='-'>
<description>-</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector0pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector0pin' terminalId='connector0terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector0pad'/><p layer='copper1' svgId='connector0pad'/></pcbView>
</views>
</connector>
<connector id='connector1' type='female' name='S'>
<description>S</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector1pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector1pin' terminalId='connector1terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector1pad'/><p layer='copper1' svgId='connector1pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
