<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-AUDIO-JACK-2.5MM">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' AUDIO-JACK 2.5MM -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>Simple 2.5mm common PCB mount audio jack. SKU: PRT-08032</description>
<title>2.5mm Audio Jack</title>
<tags>
<tag>STEREOJACK2.5MM_STEREOJACK2.5MM</tag>
<tag>2.5MM</tag>
<tag>AUDIO-JACK</tag>
</tags>
<properties>
<property name="package">stereojack2.5mm_stereojack2.5mm</property>
<property name="size">2.5mm</property>
<property name="family">sparkfun Audio Jack</property>
<property name="variant">2.5mm</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-connectors_stereojack2.5mm_stereojack2.5mm_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_audio-jack_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-connectors_stereojack2.5mm_stereojack2.5mm_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/STEREOJACK2.5MM_STEREOJACK2.5MM.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector2" name="LEFT" type="male">
<description>LEFT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pad"/>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="RIGHT" type="male">
<description>RIGHT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pad"/>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="SLEEVE" type="male">
<description>SLEEVE</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector0pad"/>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>