<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1201" moduleId="9e3cfb7c-ca08-11dd-9c4a-001f5b3a17a4">
    <version replacedby="ResistorModuleID">1</version>
    <title>100k Ω Resistor</title>
    <label>R</label>
    <date>2009-09-08</date>
    <author>Brendan Howell</author>
    <tags>
        <tag>Resistor</tag>
        <tag>basic resistor</tag>
        <tag>fritzing core</tag>
    </tags>
    <properties>
        <property name="Resistance">100kΩ</property>
        <property name="family">obsolete Resistor</property>
      <property name="Rated Power">0.25 watt</property>
      <property name="footprint">400 mil</property>
    <property name="package">THT</property></properties>
    <taxonomy>discreteParts.resistor.100000</taxonomy>
    <description>A generic resistor (0.25W)</description>
    <views>
        <iconView>
            <layers image="icon/resistor_icon_100k.svg">   
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/resistor_100k.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/resistor.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/resistor-025W.svg">
                <layer layerId="copper0"/>
                <layer layerId="keepout"/>
                <layer layerId="soldermask"/>
                <layer layerId="silkscreen"/>
                <layer layerId="outline"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="Pin 0" type="male">
            <description>Pin0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="Pin 1" type="male">
            <description>Pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>