<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Passives-CAP_POL-3528-KIT">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Passives' CAP_POL 3528-KIT -->
<version>4</version>
<date>2013-02-13</date>
<label>C</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;Capacitor Polarized&lt;/b&gt;
These are standard SMD and PTH capacitors. Normally 10uF, 47uF, and 100uF in electrolytic and tantalum varieties. Always verify the external diameter of the through hole cap, it varies with capacity, voltage, and manufacturer. The EIA devices should be standard.</description>
<title>Capacitor Polarized</title>
<tags>
<tag>EIA3528-KIT</tag>
<tag>3528-KIT</tag>
<tag>CAP_POL</tag>
</tags>
<properties>
<property name="package">eia3528-kit</property>
<property name="family">sparkfun Cap (Polarized)</property>
<property name="variant">3528-kit</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-passives_eia3528-kit_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-passives_cap_pol_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-passives_eia3528-kit_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/EIA3528-KIT.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector0" name="+" type="male">
<description>+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="-" type="male">
<description>-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>