<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Arduino_bt07'>
<version>4</version>
<date>2013-05-25</date>
<author>fabian Althaus</author>
<description>The Arduino BT is a microcontroller board originally was based on the ATmega168, but now is supplied with the 328 (datasheet) and the Bluegiga WT11 bluetooth module (details and datasheet [pdf]). It supports wireless serial communication over bluetooth (but is not compatible with Bluetooth headsets or other audio devices). It has 14 digital input/output pins (of which 6 can be used as PWM outputs and one can be used to reset the WT11 module), 6 analog inputs, a 16 MHz crystal oscillator, screw terminals for power, an ICSP header, and a reset button. It contains everything needed to support the microcontroller and can be programmed wirelessly over the Bluetooth connection. Instructions are available for getting started with the Arduino BT.</description>
<title>Arduino BT</title>
<url>http://arduino.cc/en/Main/ArduinoBoardBluetooth</url>
<tags>
<tag>Arduino</tag>
<tag>BT</tag>
<tag>Bluetooth</tag>
<tag>ATmega328</tag>
<tag>Bluegiga WT11</tag>
</tags>
<properties>
<property name='family'>microcontroller board (arduino)</property>
<property name='type'>Arduino BT (Bluetooth)</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Arduino_bt07_breadboard.svg'>
<layer layerId='breadboardbreadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Arduino_bt07_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Arduino_bt07_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Arduino_bt07_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector170' type='female' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector170pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector170pin' terminalId='connector170terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector170pad'/><p layer='copper1' svgId='connector170pad'/></pcbView>
</views>
</connector>
<connector id='connector171' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector171pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector171pin' terminalId='connector171terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector171pad'/><p layer='copper1' svgId='connector171pad'/></pcbView>
</views>
</connector>
<connector id='connector172' type='female' name='SCK/IO13'>
<description>SCK/IO13</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector172pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector172pin' terminalId='connector172terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector172pad'/><p layer='copper1' svgId='connector172pad'/></pcbView>
</views>
</connector>
<connector id='connector173' type='female' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector173pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector173pin' terminalId='connector173terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector173pad'/><p layer='copper1' svgId='connector173pad'/></pcbView>
</views>
</connector>
<connector id='connector174' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector174pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector174pin' terminalId='connector174terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector174pad'/><p layer='copper1' svgId='connector174pad'/></pcbView>
</views>
</connector>
<connector id='connector175' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector175pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector175pin' terminalId='connector175terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector175pad'/><p layer='copper1' svgId='connector175pad'/></pcbView>
</views>
</connector>
<connector id='connector176' type='female' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector176pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector176pin' terminalId='connector176terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector176pad'/><p layer='copper1' svgId='connector176pad'/></pcbView>
</views>
</connector>
<connector id='connector177' type='female' name='PWM D9'>
<description>PWM D9</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector177pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector177pin' terminalId='connector177terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector177pad'/><p layer='copper1' svgId='connector177pad'/></pcbView>
</views>
</connector>
<connector id='connector178' type='female' name='SS/PWM D10'>
<description>SS/PWM D10</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector178pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector178pin' terminalId='connector178terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector178pad'/><p layer='copper1' svgId='connector178pad'/></pcbView>
</views>
</connector>
<connector id='connector179' type='female' name='MOSI/PWM D11'>
<description>MOSI/PWM D11</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector179pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector179pin' terminalId='connector179terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector179pad'/><p layer='copper1' svgId='connector179pad'/></pcbView>
</views>
</connector>
<connector id='connector180' type='female' name='MISO/D12'>
<description>MISO/D12</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector180pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector180pin' terminalId='connector180terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector180pad'/><p layer='copper1' svgId='connector180pad'/></pcbView>
</views>
</connector>
<connector id='connector181' type='female' name='SCK/D13'>
<description>SCK/D13</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector181pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector181pin' terminalId='connector181terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector181pad'/><p layer='copper1' svgId='connector181pad'/></pcbView>
</views>
</connector>
<connector id='connector182' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector182pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector182pin' terminalId='connector182terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector182pad'/><p layer='copper1' svgId='connector182pad'/></pcbView>
</views>
</connector>
<connector id='connector183' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector183pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector183pin' terminalId='connector183terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector183pad'/><p layer='copper1' svgId='connector183pad'/></pcbView>
</views>
</connector>
<connector id='connector184' type='female' name='A4/SDA'>
<description>A4/SDA</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector184pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector184pin' terminalId='connector184terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector184pad'/><p layer='copper1' svgId='connector184pad'/></pcbView>
</views>
</connector>
<connector id='connector185' type='female' name='A5/SCL'>
<description>A5/SCL</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector185pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector185pin' terminalId='connector185terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector185pad'/><p layer='copper1' svgId='connector185pad'/></pcbView>
</views>
</connector>
<connector id='connector186' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector186pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector186pin' terminalId='connector186terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector186pad'/><p layer='copper1' svgId='connector186pad'/></pcbView>
</views>
</connector>
<connector id='connector187' type='female' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector187pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector187pin' terminalId='connector187terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector187pad'/><p layer='copper1' svgId='connector187pad'/></pcbView>
</views>
</connector>
<connector id='connector188' type='female' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector188pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector188pin' terminalId='connector188terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector188pad'/><p layer='copper1' svgId='connector188pad'/></pcbView>
</views>
</connector>
<connector id='connector189' type='female' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector189pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector189pin' terminalId='connector189terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector189pad'/><p layer='copper1' svgId='connector189pad'/></pcbView>
</views>
</connector>
<connector id='connector190' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector190pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector190pin' terminalId='connector190terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector190pad'/><p layer='copper1' svgId='connector190pad'/></pcbView>
</views>
</connector>
<connector id='connector191' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector191pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector191pin' terminalId='connector191terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector191pad'/><p layer='copper1' svgId='connector191pad'/></pcbView>
</views>
</connector>
<connector id='connector192' type='female' name='RX/D0'>
<description>RX/D0</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector192pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector192pin' terminalId='connector192terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector192pad'/><p layer='copper1' svgId='connector192pad'/></pcbView>
</views>
</connector>
<connector id='connector193' type='female' name='TX/D1'>
<description>TX/D1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector193pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector193pin' terminalId='connector193terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector193pad'/><p layer='copper1' svgId='connector193pad'/></pcbView>
</views>
</connector>
<connector id='connector194' type='female' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector194pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector194pin' terminalId='connector194terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector194pad'/><p layer='copper1' svgId='connector194pad'/></pcbView>
</views>
</connector>
<connector id='connector195' type='female' name='PWM D3'>
<description>PWM D3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector195pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector195pin' terminalId='connector195terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector195pad'/><p layer='copper1' svgId='connector195pad'/></pcbView>
</views>
</connector>
<connector id='connector196' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector196pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector196pin' terminalId='connector196terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector196pad'/><p layer='copper1' svgId='connector196pad'/></pcbView>
</views>
</connector>
<connector id='connector197' type='female' name='PWM D5'>
<description>PWM D5</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector197pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector197pin' terminalId='connector197terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector197pad'/><p layer='copper1' svgId='connector197pad'/></pcbView>
</views>
</connector>
<connector id='connector198' type='female' name='PWM D6'>
<description>PWM D6</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector198pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector198pin' terminalId='connector198terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector198pad'/><p layer='copper1' svgId='connector198pad'/></pcbView>
</views>
</connector>
<connector id='connector199' type='female' name='RESET WT11/D7'>
<description>RESET WT11/D7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector199pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector199pin' terminalId='connector199terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector199pad'/><p layer='copper1' svgId='connector199pad'/></pcbView>
</views>
</connector>
<connector id='connector200' type='female' name='JP1_1'>
<description>JP1_1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector200pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector200pin' terminalId='connector200terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector200pad'/><p layer='copper1' svgId='connector200pad'/></pcbView>
</views>
</connector>
<connector id='connector201' type='female' name='JP1_2'>
<description>JP1_2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector201pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector201pin' terminalId='connector201terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector201pad'/><p layer='copper1' svgId='connector201pad'/></pcbView>
</views>
</connector>
<connector id='connector216' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector216pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector216pin' terminalId='connector216terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector216pad'/><p layer='copper1' svgId='connector216pad'/></pcbView>
</views>
</connector>
<connector id='connector217' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector217pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector217pin' terminalId='connector217terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector217pad'/><p layer='copper1' svgId='connector217pad'/></pcbView>
</views>
</connector>
<connector id='connector218' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector218pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector218pin' terminalId='connector218terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector218pad'/><p layer='copper1' svgId='connector218pad'/></pcbView>
</views>
</connector>
<connector id='connector219' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector219pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector219pin' terminalId='connector219terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector219pad'/><p layer='copper1' svgId='connector219pad'/></pcbView>
</views>
</connector>
<connector id='connector220' type='female' name='3V3'>
<description>3V3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector220pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector220pin' terminalId='connector220terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector220pad'/><p layer='copper1' svgId='connector220pad'/></pcbView>
</views>
</connector>
<connector id='connector221' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector221pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector221pin' terminalId='connector221terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector221pad'/><p layer='copper1' svgId='connector221pad'/></pcbView>
</views>
</connector>
<connector id='connector222' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector222pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector222pin' terminalId='connector222terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector222pad'/><p layer='copper1' svgId='connector222pad'/></pcbView>
</views>
</connector>
<connector id='connector223' type='female' name='N/C'>
<description>N/C</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector223pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector223pin' terminalId='connector223terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector223pad'/><p layer='copper1' svgId='connector223pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='mosi'>
<nodeMember connectorId='connector173'/>
<nodeMember connectorId='connector179'/>
</bus>
<bus id='miso'>
<nodeMember connectorId='connector170'/>
<nodeMember connectorId='connector180'/>
</bus>
<bus id='sck/io13'>
<nodeMember connectorId='connector172'/>
<nodeMember connectorId='connector181'/>
</bus>
<bus id='gnd'>
<nodeMember connectorId='connector175'/>
<nodeMember connectorId='connector182'/>
<nodeMember connectorId='connector217'/>
<nodeMember connectorId='connector218'/>
</bus>
<bus id='ad4/sda'>
<nodeMember connectorId='connector184'/>
<nodeMember connectorId='connector190'/>
</bus>
<bus id='ad5/scl'>
<nodeMember connectorId='connector185'/>
<nodeMember connectorId='connector191'/>
</bus>
<bus id='+5v'>
<nodeMember connectorId='connector171'/>
<nodeMember connectorId='connector219'/>
<nodeMember connectorId='connector222'/>
</bus>
<bus id='reset'>
<nodeMember connectorId='connector174'/>
<nodeMember connectorId='connector221'/>
</bus>
</buses>
</module>
