<?xml version="1.0" encoding="UTF-8"?><module moduleId="3234DBDC80leg">
 <version>4</version>
 <author>Stefan Hermann</author>
 <title>Basic Servo</title>
 <label>J</label>
 <date>2008-11-04</date>
 <tags>
  <tag>servo</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">Servo</property>
 </properties>
 <taxonomy>discreteParts.servo</taxonomy>
 <description>A generic servo.</description>
 <views>
  <iconView>
   <layers image="icon/basic_servo.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/servo.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/servo_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/jumper_3_100mil_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="gnd" type="male">
   <description>ground</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="vcc" type="male">
   <description>vcc</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" legId="connector1leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector2" name="pulse" type="male">
   <description>pulse</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin" legId="connector2leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
    <p layer="copper1" svgId="connector2pin"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>