<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.3.21b.04.28.4164" moduleId="371230f4269dfda53ae3cc123cd5fdb4">
<version replacedby="Arduino-Mini-v5">5</version>
    <author>Lionel Michel</author>
    <title>Arduino Mini</title>
    <label>Arduino</label>
    <date>2010-04-30</date>
    <tags>
        <tag>Arduino</tag>
        <tag>Mini</tag>
        <tag>microcontroller</tag>
        <tag>fritzing core</tag>
    </tags>
    <properties>
        <property name="family">/obsolete/Microcontroller Board (Arduino)</property>
        <property name="processor">ATmega</property>
        <property name="variant">Arduino Mini</property>
   </properties>
    <description>
    The Arduino Mini is a small microcontroller board based on the ATmega168 (datasheet), intended for use on breadboards and when space is at a premium. It has 14 digital input/output pins (of which 6 can be used as PWM outputs), 8 analog inputs, and a 16 MHz crystal oscillator. It can be programmed with the Mini USB adapter or other USB or RS232 to TTL serial adapter.
    
    http://arduino.cc/en/Main/ArduinoBoardMini</description>
    <views>
        <iconView>
            <layers image="icon/Arduino_Mini.svg">
                <layer layerId="icon" />
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/controller_arduino_mini.svg">
                <layer layerId="breadboard" />
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/controller_arduino_mini.svg">
                <layer layerId="schematic" />
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/pcb-arduino-mini.svg">
                <layer layerId="copper0" />
                <layer layerId="copper1" />
                <layer layerId="silkscreen" />
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector15" name="+5V" replacedby="connector56" type="female">
            <description>+5 V Regulated DC</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pin" />
                   <p layer="copper1" svgId="connector15pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" name="A1" type="male">
            <description>Analog Input 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pin" />
                    <p layer="copper1" svgId="connector7pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" name="D1" replacedby="connector55" type="female">
            <description>Digital I/O 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector16pin" />
                    <p layer="copper1" svgId="connector16pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" name="A2" type="male">
            <description>Analog Input 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pin" />
                    <p layer="copper1" svgId="connector8pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" name="D0" replacedby="connector54" type="female">
            <description>Digital I/O 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector17pin" />
                    <p layer="copper1" svgId="connector17pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" name="A3" type="male">
            <description>Analog Input 3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector9pin" />
                    <p layer="copper1" svgId="connector9pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" name="D7" type="female" replacedby="connector53">
            <description>Digital I/O 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector18pin" />
                   <p layer="copper1" svgId="connector18pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" name="D0" replacedby="connector25" type="male">
            <description>Digital I/O 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector19pin" />
                    <p layer="copper1" svgId="connector19pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector20" name="D1" replacedby="connector26" type="male">
            <description>Digital I/O 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector20pin" />
                    <p layer="copper1" svgId="connector20pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" name="RST" replacedby="connector27" type="male">
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector21pin" />
                    <p layer="copper1" svgId="connector21pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" name="GND" replacedby="connector28" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector22pin" />
                    <p layer="copper1" svgId="connector22pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" name="D2" type="male">
            <description>Digital I/O 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector23pin" />
                    <p layer="copper1" svgId="connector23pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector24" name="D3" replacedby="connector30" type="male">
            <description>Digital I/O 3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector24pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector24pin" terminalId="connector24terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector24pin" />
                     <p layer="copper1" svgId="connector24pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector25" name="D4" type="male">
            <description>Digital I/O 4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector25pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector25pin" terminalId="connector25terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector25pin" />
                    <p layer="copper1" svgId="connector25pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector26" name="D5" replacedby="connector32" type="male">
            <description>Digital I/O 5</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector26pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector26pin" terminalId="connector26terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector26pin" />
                     <p layer="copper1" svgId="connector26pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector27" name="D6" replacedby="connector33" type="male">
            <description>Digital I/O 6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector27pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector27pin" terminalId="connector27terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector27pin" />
                    <p layer="copper1" svgId="connector27pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector28" name="D7" type="male" replacedby="connector53">
            <description>Digital I/O 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector28pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector28pin" terminalId="connector28terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector28pin" />
                    <p layer="copper1" svgId="connector28pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector29" name="D8" type="male">
            <description>Digital I/O 8</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector29pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector29pin" terminalId="connector29terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector29pin" />
                     <p layer="copper1" svgId="connector29pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector30" name="D9" replacedby="connector36" type="male">
            <description>Digital I/O 9</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector30pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector30pin" terminalId="connector30terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector30pin" />
                    <p layer="copper1" svgId="connector30pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector31" name="A6" replacedby="connector49" type="female">
            <description>Analog Input 6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector31pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector31pin" terminalId="connector31terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector31pin" />
                   <p layer="copper1" svgId="connector31pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector32" name="A7" replacedby="connector51" type="female">
            <description>Analog Input 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector32pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector32pin" terminalId="connector32terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector32pin" />
                    <p layer="copper1" svgId="connector32pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector33" name="A4" replacedby="connector50" type="female">
            <description>Analog Input 4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector33pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector33pin" terminalId="connector33terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector33pin" />
                    <p layer="copper1" svgId="connector33pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" name="+5V" replacedby="connector59" type="female">
            <description>+5 V Regulated DC</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin" />
                      <p layer="copper1" svgId="connector0pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector34" name="A5" replacedby="connector52" type="female">
            <description>Analog Input 5</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector34pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector34pin" terminalId="connector34terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector34pin" />
                   <p layer="copper1" svgId="connector34pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="GND" replacedby="connector58" type="female">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin" />
                     <p layer="copper1" svgId="connector1pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" name="D10" replacedby="connector48" type="male">
            <description>Digital I/O 10</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin" />
                    <p layer="copper1" svgId="connector2pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" name="+5V" replacedby="connector40" type="male">
            <description>+5 V Regulated DC</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pin" />
                    <p layer="copper1" svgId="connector10pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" name="D11" replacedby="connector47" type="male">
            <description>Digital I/O 11</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin" />
                    <p layer="copper1" svgId="connector3pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" name="RST" replacedby="connector39" type="male">
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pin" />
                   <p layer="copper1" svgId="connector11pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" name="D12" type="male">
            <description>Digital I/O 12</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin" />
                    <p layer="copper1" svgId="connector4pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" name="GND" replacedby="connector38" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pin" />
                    <p layer="copper1" svgId="connector12pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" name="D13" type="male">
            <description>Digital I/O 13</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin" />
                    <p layer="copper1" svgId="connector5pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" name="+9V" replacedby="connector37" type="male">
            <description>+9 V Regulated DC</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pin" />
                    <p layer="copper1" svgId="connector13pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" name="A0" type="male">
            <description>Analog Input 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pin" />
                    <p layer="copper1" svgId="connector6pin" />
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" name="GND" replacedby="connector57" type="female">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal" />
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector14pin" />
                    <p layer="copper1" svgId="connector14pin" />
                </pcbView>
            </views>
        </connector>
    </connectors>
	<buses>
		<bus id="GND">
			<nodeMember connectorId="connector22" />
			<nodeMember connectorId="connector1" />
			<nodeMember connectorId="connector12" />
			<nodeMember connectorId="connector14" />
		</bus>
		<bus id="D0">
			<nodeMember connectorId="connector17" />
			<nodeMember connectorId="connector19" />
		</bus>
		<bus id="D1">
			<nodeMember connectorId="connector20" />
			<nodeMember connectorId="connector16" />
		</bus>
		<bus id="5V">
			<nodeMember connectorId="connector15" />
			<nodeMember connectorId="connector0" />
			<nodeMember connectorId="connector10" />
		</bus>
		<bus id="RST">
			<nodeMember connectorId="connector11" />
			<nodeMember connectorId="connector21" />
			</bus>
		</buses>
</module>