<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.2.2.b.03.04.2550" moduleId="f9f8ddcf-1edf-11de-8283-0019d2b7521e">
<version replacedby="generic_female_pin_header_3_100mil">1</version>
    <author>Fritzing Part-o-matic</author>
    <title>Generic female header - 3 pins</title>
    <label>J</label>
    <date>2009-10-01</date>
    <tags/>
    <properties>
        <property name="family">obsolete Pin Header</property>
        <property name="Pins">3</property>
        <property name="Gender">♀</property>
        <property name="Pin Spacing">0.1in (2.54mm)</property>
        <property name="Hole Shape">Square</property>
    <property name="package">THT</property></properties>
    <description>Generic female header</description>
    <views>
        <iconView>
            <layers image="icon/generic_female_header.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/generic-female-header_bread_3.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/generic-female-header_schem_3.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/jumper3.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="pin1" type="male">
            <description>Pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="pin2" type="male">
            <description>Pin 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" name="pin3" type="male">
            <description>Pin 3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>