<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='ProtoShield-Mini-v12'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;strong&gt;Description: &lt;/strong&gt;This is a small prototyping shield for the Arduino Pro Mini. If your project requires just a little bit more space for your external circuitry, this might be a perfect addition. 38 unconnected PTHs are provided for your prototyping needs.&lt;/p&gt;


&lt;p&gt;


	The shield fits the small form factor of the Arduino Pro Mini - connecting to the &amp;#39;top&amp;#39; four pins on each side of the Mini (&amp;#39;GND&amp;#39;-&amp;#39;TXO&amp;#39; &amp;amp; &amp;#39;VCC&amp;#39;-&amp;#39;RAW&amp;#39;). There are small buses for VCC, GND and RAW. In addition to the power buses, the serial pins are also broken out on the shield. The analog and digital pins are not broken out on the shield.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Features:&lt;/strong&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		VCC, RAW and GND buses&lt;/li&gt;


	&lt;li&gt;


		Serial (RXI &amp;amp; TXO) pins broken out to small buses&lt;/li&gt;


	&lt;li&gt;


		Works with both 5V and 3.3V Pro Mini versions&lt;/li&gt;


	&lt;li&gt;


		Upholds the Pro Mini&amp;#39;s small form factor&lt;/li&gt;


	&lt;li&gt;


		38 unconnected PTHs for prototyping&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Arduino Mini Proto Shield</title>
<url>http://www.sparkfun.com/products/9709</url>
<tags>
<tag>Arduino</tag>
<tag>Mini</tag>
<tag>Proto</tag>
</tags>
<properties>
<property name='family'>Prototype Shield</property>
<property name='Shield Size'>Mini</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/ProtoShield-Mini-v12_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/ProtoShield-Mini-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/ProtoShield-Mini-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/ProtoShield-Mini-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector0' type='male' name='GND1'>
<description>GND1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector0pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector0pin' terminalId='connector0terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector0pad'/><p layer='copper1' svgId='connector0pad'/></pcbView>
</views>
</connector>
<connector id='connector1' type='male' name='2'>
<description>2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector1pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector1pin' terminalId='connector1terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector1pad'/><p layer='copper1' svgId='connector1pad'/></pcbView>
</views>
</connector>
<connector id='connector2' type='male' name='RXI'>
<description>RXI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector2pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector2pin' terminalId='connector2terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector2pad'/><p layer='copper1' svgId='connector2pad'/></pcbView>
</views>
</connector>
<connector id='connector3' type='male' name='TXO'>
<description>TXO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector3pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector3pin' terminalId='connector3terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector3pad'/><p layer='copper1' svgId='connector3pad'/></pcbView>
</views>
</connector>
<connector id='connector4' type='male' name='RAW'>
<description>RAW</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector4pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector4pin' terminalId='connector4terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector4pad'/><p layer='copper1' svgId='connector4pad'/></pcbView>
</views>
</connector>
<connector id='connector5' type='male' name='GND2'>
<description>GND2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector5pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector5pin' terminalId='connector5terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector5pad'/><p layer='copper1' svgId='connector5pad'/></pcbView>
</views>
</connector>
<connector id='connector6' type='male' name='3'>
<description>3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
<connector id='connector8' type='female' name='GND1'>
<description>GND1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad' hybrid='yes' /><p layer='copper1' svgId='connector8pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector9' type='female' name='GND1'>
<description>GND1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad' hybrid='yes' /><p layer='copper1' svgId='connector9pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector10' type='female' name='GND1'>
<description>GND1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad' hybrid='yes' /><p layer='copper1' svgId='connector10pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector11' type='female' name='GND1'>
<description>GND1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad' hybrid='yes' /><p layer='copper1' svgId='connector11pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector12' type='female' name='GND1'>
<description>GND1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad' hybrid='yes' /><p layer='copper1' svgId='connector12pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector13' type='female' name='GND2'>
<description>GND2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad' hybrid='yes' /><p layer='copper1' svgId='connector13pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector14' type='female' name='GND2'>
<description>GND2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad' hybrid='yes' /><p layer='copper1' svgId='connector14pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector15' type='female' name='N$1'>
<description>N$1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad' hybrid='yes' /><p layer='copper1' svgId='connector15pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector16' type='female' name='N$2'>
<description>N$2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad' hybrid='yes' /><p layer='copper1' svgId='connector16pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector17' type='female' name='N$3'>
<description>N$3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad' hybrid='yes' /><p layer='copper1' svgId='connector17pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector18' type='female' name='N$4'>
<description>N$4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector18pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector18pin' terminalId='connector18terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector18pad' hybrid='yes' /><p layer='copper1' svgId='connector18pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector19' type='female' name='N$5'>
<description>N$5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector19pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector19pin' terminalId='connector19terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector19pad' hybrid='yes' /><p layer='copper1' svgId='connector19pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector20' type='female' name='N$6'>
<description>N$6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector20pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector20pin' terminalId='connector20terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector20pad' hybrid='yes' /><p layer='copper1' svgId='connector20pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector21' type='female' name='N$7'>
<description>N$7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector21pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector21pin' terminalId='connector21terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector21pad' hybrid='yes' /><p layer='copper1' svgId='connector21pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector22' type='female' name='N$8'>
<description>N$8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad' hybrid='yes' /><p layer='copper1' svgId='connector22pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector23' type='female' name='N$9'>
<description>N$9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad' hybrid='yes' /><p layer='copper1' svgId='connector23pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector24' type='female' name='N$10'>
<description>N$10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad' hybrid='yes' /><p layer='copper1' svgId='connector24pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector25' type='female' name='N$11'>
<description>N$11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad' hybrid='yes' /><p layer='copper1' svgId='connector25pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector26' type='female' name='N$12'>
<description>N$12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad' hybrid='yes' /><p layer='copper1' svgId='connector26pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector27' type='female' name='N$13'>
<description>N$13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad' hybrid='yes' /><p layer='copper1' svgId='connector27pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector28' type='female' name='N$14'>
<description>N$14</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad' hybrid='yes' /><p layer='copper1' svgId='connector28pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector29' type='female' name='N$15'>
<description>N$15</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad' hybrid='yes' /><p layer='copper1' svgId='connector29pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector30' type='female' name='N$16'>
<description>N$16</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad' hybrid='yes' /><p layer='copper1' svgId='connector30pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector31' type='female' name='N$17'>
<description>N$17</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad' hybrid='yes' /><p layer='copper1' svgId='connector31pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector32' type='female' name='N$18'>
<description>N$18</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad' hybrid='yes' /><p layer='copper1' svgId='connector32pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector33' type='female' name='N$19'>
<description>N$19</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad' hybrid='yes' /><p layer='copper1' svgId='connector33pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector34' type='female' name='N$20'>
<description>N$20</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad' hybrid='yes' /><p layer='copper1' svgId='connector34pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector35' type='female' name='N$21'>
<description>N$21</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad' hybrid='yes' /><p layer='copper1' svgId='connector35pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector36' type='female' name='N$22'>
<description>N$22</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad' hybrid='yes' /><p layer='copper1' svgId='connector36pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector37' type='female' name='N$23'>
<description>N$23</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad' hybrid='yes' /><p layer='copper1' svgId='connector37pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector38' type='female' name='N$24'>
<description>N$24</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad' hybrid='yes' /><p layer='copper1' svgId='connector38pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector39' type='female' name='N$25'>
<description>N$25</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad' hybrid='yes' /><p layer='copper1' svgId='connector39pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector40' type='female' name='N$26'>
<description>N$26</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad' hybrid='yes' /><p layer='copper1' svgId='connector40pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector41' type='female' name='N$28'>
<description>N$28</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad' hybrid='yes' /><p layer='copper1' svgId='connector41pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector42' type='female' name='N$29'>
<description>N$29</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad' hybrid='yes' /><p layer='copper1' svgId='connector42pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector43' type='female' name='N$30'>
<description>N$30</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad' hybrid='yes' /><p layer='copper1' svgId='connector43pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector44' type='female' name='N$31'>
<description>N$31</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad' hybrid='yes' /><p layer='copper1' svgId='connector44pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector45' type='female' name='N$32'>
<description>N$32</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad' hybrid='yes' /><p layer='copper1' svgId='connector45pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector46' type='female' name='N$33'>
<description>N$33</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector46pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector46pin' terminalId='connector46terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector46pad' hybrid='yes' /><p layer='copper1' svgId='connector46pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector47' type='female' name='N$34'>
<description>N$34</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector47pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector47pin' terminalId='connector47terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector47pad' hybrid='yes' /><p layer='copper1' svgId='connector47pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector48' type='female' name='N$42'>
<description>N$42</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector48pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector48pin' terminalId='connector48terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector48pad' hybrid='yes' /><p layer='copper1' svgId='connector48pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector49' type='female' name='N$43'>
<description>N$43</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector49pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector49pin' terminalId='connector49terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector49pad' hybrid='yes' /><p layer='copper1' svgId='connector49pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector50' type='female' name='N$44'>
<description>N$44</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector50pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector50pin' terminalId='connector50terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector50pad' hybrid='yes' /><p layer='copper1' svgId='connector50pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector51' type='female' name='N$45'>
<description>N$45</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector51pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector51pin' terminalId='connector51terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector51pad' hybrid='yes' /><p layer='copper1' svgId='connector51pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector52' type='female' name='N$46'>
<description>N$46</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector52pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector52pin' terminalId='connector52terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector52pad' hybrid='yes' /><p layer='copper1' svgId='connector52pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector53' type='female' name='RAW'>
<description>RAW</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector53pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector53pin' terminalId='connector53terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector53pad' hybrid='yes' /><p layer='copper1' svgId='connector53pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector54' type='female' name='RAW'>
<description>RAW</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector54pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector54pin' terminalId='connector54terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector54pad' hybrid='yes' /><p layer='copper1' svgId='connector54pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector55' type='female' name='RXI'>
<description>RXI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector55pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector55pin' terminalId='connector55terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector55pad' hybrid='yes' /><p layer='copper1' svgId='connector55pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector56' type='female' name='RXI'>
<description>RXI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector56pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector56pin' terminalId='connector56terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector56pad' hybrid='yes' /><p layer='copper1' svgId='connector56pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector57' type='female' name='TXO'>
<description>TXO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector57pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector57pin' terminalId='connector57terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector57pad' hybrid='yes' /><p layer='copper1' svgId='connector57pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector58' type='female' name='TXO'>
<description>TXO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector58pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector58pin' terminalId='connector58terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector58pad' hybrid='yes' /><p layer='copper1' svgId='connector58pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector59' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector59pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector59pin' terminalId='connector59terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector59pad' hybrid='yes' /><p layer='copper1' svgId='connector59pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector60' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector60pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector60pin' terminalId='connector60terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector60pad' hybrid='yes' /><p layer='copper1' svgId='connector60pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector61' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector61pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector61pin' terminalId='connector61terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector61pad' hybrid='yes' /><p layer='copper1' svgId='connector61pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector62' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector62pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector62pin' terminalId='connector62terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector62pad' hybrid='yes' /><p layer='copper1' svgId='connector62pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector63' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector63pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector63pin' terminalId='connector63terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector63pad' hybrid='yes' /><p layer='copper1' svgId='connector63pad' hybrid='yes' /></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
