<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Sensors-MLX90614-_">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Sensors' MLX90614 _ -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>Non-contact PIR I2C interface temperature sensor</description>
<title>MLX90614</title>
<tags>
<tag>TO-39</tag>
<tag>MLX90614</tag>
<tag>_</tag>
</tags>
<properties>
<property name="package">to-39</property>
<property name="family">sparkfun Temperature Sensor</property>
<property name="features">non-contact</property>
<property name="interface">I2C</property>
<property name="variant">_</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-sensors_to-39_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-sensors_mlx90614_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-sensors_to-39_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/TO-39.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector1" name="PWM_SDA" type="male">
<description>PWM_SDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector1pad"/>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="SCL_VZ" type="male">
<description>SCL_VZ</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector0pad"/>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pad"/>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="VSS" type="male">
<description>VSS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pad"/>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>