<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.18" moduleId="37asdf3c843a2127a0e499f8a0b3ef6a">
<version replacedby="37asdf3c843a2127a0e499f8a0b3ef6aCrystalModuleID">4</version>
    <author>André Knörig</author>
    <title>Resonator</title>
    <label>Y</label>
    <date>2010-03-06</date>
    <tags>
        <tag>clock</tag>
        <tag>resonator</tag>
        <tag>oscillator</tag>
        <tag>ceramic</tag>
    </tags>
    <properties>
        <property name="family">obsolete oscillator</property>
        <property name="type">ceramic resonator with capacitor</property>
        <property name="frequency" showInLabel="yes">16 Mhz</property>
    <property name="package">THT</property></properties>
    <description>Ceramic resonator with built-in capacitors</description>
    <views>
        <iconView>
            <layers image="icon/resonator-3pin.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/resonator-3pin.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <pcbView>
            <layers image="pcb/resonator-3pin.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
        <schematicView>
            <layers image="schematic/resonator-3pin.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
    </views>
    <connectors>
        <connector id="connector0" name="0" type="male">
            <description>Pin 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="GND" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector2" name="pin 1" type="male">
            <description>Pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                <p layer="copper1" svgId="connector2pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>