<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-RF-RN-131G-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-RF' RN-131G  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>Roving Netowrks WiFLy GSX Module</description>
<title>RN-131G</title>
<tags>
<tag>RN-131G</tag>
</tags>
<properties>
<property name="package">rn-131g</property>
<property name="family">sparkfun GSX Module</property>
<property name="chip">RN-131G</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-rf_rn-131g_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-rf_rn-131g_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-rf_rn-131g_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/RN-131G.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector17" name="3.3V-RIN" type="male">
<description>3.3V-RIN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector16" name="3.3V-ROUT" type="male">
<description>3.3V-ROUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector16pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector16pad"/>
</pcbView>
</views>
</connector>
<connector id="connector14" name="CLK" type="male">
<description>CLK</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector14pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector14pad"/>
</pcbView>
</views>
</connector>
<connector id="connector22" name="DMA-RX" type="male">
<description>DMA-RX</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector22pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector22pad"/>
</pcbView>
</views>
</connector>
<connector id="connector21" name="DMA-TX" type="male">
<description>DMA-TX</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector21pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector21pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="EPC-A" type="male">
<description>EPC-A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="EPC-B" type="male">
<description>EPC-B</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="F_AWAKE" type="male">
<description>F_AWAKE</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector18" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector18pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector18pad"/>
</pcbView>
</views>
</connector>
<connector id="connector35" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector35pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector35pin" terminalId="connector35terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector35pad"/>
</pcbView>
</views>
</connector>
<connector id="connector36" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector36pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector36pin" terminalId="connector36terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector36pad"/>
</pcbView>
</views>
</connector>
<connector id="connector37" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector37pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector37pin" terminalId="connector37terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector37pad"/>
</pcbView>
</views>
</connector>
<connector id="connector38" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector38pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector38pin" terminalId="connector38terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector38pad"/>
</pcbView>
</views>
</connector>
<connector id="connector39" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector39pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector39pin" terminalId="connector39terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector39pad"/>
</pcbView>
</views>
</connector>
<connector id="connector40" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector40pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector40pin" terminalId="connector40terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector40pad"/>
</pcbView>
</views>
</connector>
<connector id="connector41" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector41pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector41pin" terminalId="connector41terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector41pad"/>
</pcbView>
</views>
</connector>
<connector id="connector42" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector42pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector42pin" terminalId="connector42terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector42pad"/>
</pcbView>
</views>
</connector>
<connector id="connector43" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector43pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector43pin" terminalId="connector43terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector43pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="GPIO-12" type="male">
<description>GPIO-12</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="GPIO-13" type="male">
<description>GPIO-13</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector28" name="GPIO-4" type="male">
<description>GPIO-4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector28pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector28pad"/>
</pcbView>
</views>
</connector>
<connector id="connector27" name="GPIO-5" type="male">
<description>GPIO-5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector27pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector27pad"/>
</pcbView>
</views>
</connector>
<connector id="connector26" name="GPIO-6" type="male">
<description>GPIO-6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector26pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector26pad"/>
</pcbView>
</views>
</connector>
<connector id="connector25" name="GPIO-7" type="male">
<description>GPIO-7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector25pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector25pad"/>
</pcbView>
</views>
</connector>
<connector id="connector24" name="GPIO-8" type="male">
<description>GPIO-8</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector24pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector24pad"/>
</pcbView>
</views>
</connector>
<connector id="connector23" name="GPIO-9" type="male">
<description>GPIO-9</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector23pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector23pad"/>
</pcbView>
</views>
</connector>
<connector id="connector15" name="MISO" type="male">
<description>MISO</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector15pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector15pad"/>
</pcbView>
</views>
</connector>
<connector id="connector13" name="MOSI" type="male">
<description>MOSI</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="RESET" type="male">
<description>RESET</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="RX" type="male">
<description>RX</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector33" name="SEN0" type="male">
<description>SEN0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector33pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector33pin" terminalId="connector33terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector33pad"/>
</pcbView>
</views>
</connector>
<connector id="connector29" name="SEN1" type="male">
<description>SEN1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector29pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector29pad"/>
</pcbView>
</views>
</connector>
<connector id="connector30" name="SEN2" type="male">
<description>SEN2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector30pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector30pin" terminalId="connector30terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector30pad"/>
</pcbView>
</views>
</connector>
<connector id="connector31" name="SEN3" type="male">
<description>SEN3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector31pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector31pin" terminalId="connector31terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector31pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="SEN4" type="male">
<description>SEN4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="SEN5" type="male">
<description>SEN5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="SEN6" type="male">
<description>SEN6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="SEN7" type="male">
<description>SEN7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector32" name="SENSE-PWR" type="male">
<description>SENSE-PWR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector32pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector32pin" terminalId="connector32terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector32pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="S_CAP" type="male">
<description>S_CAP</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="TX" type="male">
<description>TX</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector19" name="VDD-BATT" type="male">
<description>VDD-BATT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector19pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector19pad"/>
</pcbView>
</views>
</connector>
<connector id="connector20" name="VDD-IN" type="male">
<description>VDD-IN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector20pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector20pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="GND">
<nodeMember connectorId="connector43"/>
<nodeMember connectorId="connector42"/>
<nodeMember connectorId="connector41"/>
<nodeMember connectorId="connector40"/>
<nodeMember connectorId="connector39"/>
<nodeMember connectorId="connector38"/>
<nodeMember connectorId="connector37"/>
<nodeMember connectorId="connector36"/>
<nodeMember connectorId="connector35"/>
<nodeMember connectorId="connector18"/>
</bus>
</buses>
</module>