<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1201" moduleId="2012BCEC1FB">
 <version replacedby="2012BCEC1FBThermistorModuleID">4</version>
 <author>Brendan Howell</author>
 <title>Temperature Sensor (Thermistor)</title>
 <label>R</label>
 <date>2009-01-07</date>
 <tags>
  <tag>Thermistor</tag>
  <tag>Temperature Sensor</tag>
  <tag>fritzing core</tag>
  <tag>sensor</tag>
  <tag>heat sensor</tag>
 </tags>
 <properties>
  <property name="family">obsolete Thermistor</property>
  <property name="Resistance at 25°">10k&#937;</property>
  <property name="Thermistor Type">NTC (Negative Temperature Coefficient)</property>
 <property name="package">THT</property></properties>
 <taxonomy>discreteParts.sensor.heat.thermistor</taxonomy>
 <description>A 10k NTC Thermistor (Temperature Sensor)</description>
 <views>
  <iconView>
   <layers image="icon/ceramic_disk_thermistor.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView fliphorizontal="true" flipvertical="true">
   <layers image="breadboard/ceramic_disk_thermistor.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/thermistor.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/axial_lay_2_300mil_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="pin 0" type="male">
   <description>pin0</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="pin 1" type="male">
   <description>pin1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>