<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.5.2b.02.18.4756" moduleId="SPARKCORE_v1" referenceFile="SPARKCORE_v1.fzp">
 <version replacedby="SPARKCORE_v1_fix">5</version>
 <date>Wed Jan 22 2014</date>
 <author>BDub @ Technobly.com</author>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:7.8pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">The Spark Core is a tiny Wi-Fi development board that makes it easy to create internet-connected hardware. The Core is all you need to get started; power it over USB and in minutes you'll be controlling LEDs, switches and motors and collecting data from sensors over the internet!&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">It has 8 digital I/O pins, 8 analog I/O pins, 8 PWM pins; UART (Serial), SPI, I2C, and JTAG peripherals available. Programmed wirelessly (through Spark Cloud), via USB or JTAG. 3.3VDC supply voltage (on board power regulator); can be powered by USB Micro 100mA typical current consumption; 300mA peak consumption (during transmit events). 2MB of external flash; EEPROM supplied by CC3000. STM32F103 microcontroller, ARM Cortex M3 architecture, 32-bit 72Mhz processor, 128KB of Flash, 20KB of RAM.&lt;/p>&lt;/body>&lt;/html></description>
 <title>Spark Core (v1.0)</title>
 <url>http://spark.io</url>
 <tags>
  <tag>Arduino Compatible</tag>
  <tag>Spark Core</tag>
  <tag>Wifi</tag>
  <tag>STM32F103</tag>
  <tag>Development Platform</tag>
  <tag>CC3000</tag>
 </tags>
 <properties>
  <property name="family">//obsolete//microcontroller board (arduino compatible)</property>
  <property name="variant">variant 1</property>
  <property name="revision">v1.0</property>
  <property name="layer"></property>
  <property name="manufacturer">Spark Devices</property>
  <property name="name">Spark Core</property>
  <property name="part number"></property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/SPARKCORE_v1_breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/SPARKCORE_v1_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/SPARKCORE_v1_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/SPARKCORE_v1_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="male" id="connector41" name="A0">
   <description>Analog Input 0 / PWM1</description>
   <views>
    <breadboardView>
     <p svgId="connector41pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector41pin" layer="schematic" terminalId="connector41terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector41pad" layer="copper0"/>
     <p svgId="connector41pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector42" name="A1">
   <description>Analog Input 1 / PWM2</description>
   <views>
    <breadboardView>
     <p svgId="connector42pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector42pin" layer="schematic" terminalId="connector42terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector42pad" layer="copper0"/>
     <p svgId="connector42pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector43" name="A2">
   <description>Analog Input 2 / SS (SPI)</description>
   <views>
    <breadboardView>
     <p svgId="connector43pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector43pin" layer="schematic" terminalId="connector43terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector43pad" layer="copper0"/>
     <p svgId="connector43pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector44" name="A3">
   <description>Analog Input 3 / SCK (SPI)</description>
   <views>
    <breadboardView>
     <p svgId="connector44pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector44pin" layer="schematic" terminalId="connector44terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector44pad" layer="copper0"/>
     <p svgId="connector44pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector45" name="A4">
   <description>Analog Input 4 / PWM3 / MISO (SPI)</description>
   <views>
    <breadboardView>
     <p svgId="connector45pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector45pin" layer="schematic" terminalId="connector45terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector45pad" layer="copper0"/>
     <p svgId="connector45pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector46" name="A5">
   <description>Analog Input 5 / PWM4 / MOSI (SPI)</description>
   <views>
    <breadboardView>
     <p svgId="connector46pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector46pin" layer="schematic" terminalId="connector46terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector46pad" layer="copper0"/>
     <p svgId="connector46pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector47" name="A6">
   <description>Analog Input 6 / PWM5</description>
   <views>
    <breadboardView>
     <p svgId="connector47pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector47pin" layer="schematic" terminalId="connector47terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector47pad" layer="copper0"/>
     <p svgId="connector47pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector48" name="A7">
   <description>Analog Input 7 / PWM6</description>
   <views>
    <breadboardView>
     <p svgId="connector48pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector48pin" layer="schematic" terminalId="connector48terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector48pad" layer="copper0"/>
     <p svgId="connector48pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector49" name="TX">
   <description>Serial1 UART Transmit</description>
   <views>
    <breadboardView>
     <p svgId="connector49pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector49pin" layer="schematic" terminalId="connector49terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector49pad" layer="copper0"/>
     <p svgId="connector49pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector50" name="RX">
   <description>Serial1 UART Receive</description>
   <views>
    <breadboardView>
     <p svgId="connector50pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector50pin" layer="schematic" terminalId="connector50terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector50pad" layer="copper0"/>
     <p svgId="connector50pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector51" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector51pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector51pin" layer="schematic" terminalId="connector51terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector51pad" layer="copper0"/>
     <p svgId="connector51pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector52" name="VIN">
   <description>Diode drop below USB V+ / Input to 3.3V Regulator (3.6 - 6V max input)</description>
   <views>
    <breadboardView>
     <p svgId="connector52pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector52pin" layer="schematic" terminalId="connector52terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector52pad" layer="copper0"/>
     <p svgId="connector52pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector53" name="D0">
   <description>Digital Input/Output 0 / SDA (ISC) / PWM7</description>
   <views>
    <breadboardView>
     <p svgId="connector53pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector53pin" layer="schematic" terminalId="connector53terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector53pad" layer="copper0"/>
     <p svgId="connector53pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector54" name="D1">
   <description>Digital Input/Output 1 / SCL (I2C) / PWM8</description>
   <views>
    <breadboardView>
     <p svgId="connector54pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector54pin" layer="schematic" terminalId="connector54terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector54pad" layer="copper0"/>
     <p svgId="connector54pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector55" name="D2">
   <description>Digital Input/Output 2</description>
   <views>
    <breadboardView>
     <p svgId="connector55pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector55pin" layer="schematic" terminalId="connector55terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector55pad" layer="copper0"/>
     <p svgId="connector55pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector56" name="D3">
   <description>Digital Input/Output 3</description>
   <views>
    <breadboardView>
     <p svgId="connector56pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector56pin" layer="schematic" terminalId="connector56terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector56pad" layer="copper0"/>
     <p svgId="connector56pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector57" name="D4">
   <description>Digital Input/Output 4</description>
   <views>
    <breadboardView>
     <p svgId="connector57pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector57pin" layer="schematic" terminalId="connector57terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector57pad" layer="copper0"/>
     <p svgId="connector57pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector58" name="D5">
   <description>Digital Input/Output 5</description>
   <views>
    <breadboardView>
     <p svgId="connector58pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector58pin" layer="schematic" terminalId="connector58terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector58pad" layer="copper0"/>
     <p svgId="connector58pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector59" name="D6">
   <description>Digital Input/Output 6</description>
   <views>
    <breadboardView>
     <p svgId="connector59pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector59pin" layer="schematic" terminalId="connector59terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector59pad" layer="copper0"/>
     <p svgId="connector59pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector60" name="D7">
   <description>Digital Input/Output 7</description>
   <views>
    <breadboardView>
     <p svgId="connector60pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector60pin" layer="schematic" terminalId="connector60terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector60pad" layer="copper0"/>
     <p svgId="connector60pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector61" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector61pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector61pin" layer="schematic" terminalId="connector61terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector61pad" layer="copper0"/>
     <p svgId="connector61pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector62" name="3V3*">
   <description>Filtered 3.3V Output (Aref input)</description>
   <views>
    <breadboardView>
     <p svgId="connector62pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector62pin" layer="schematic" terminalId="connector62terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector62pad" layer="copper0"/>
     <p svgId="connector62pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector63" name="RST">
   <description>Reset Input (Active Low)</description>
   <views>
    <breadboardView>
     <p svgId="connector63pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector63pin" layer="schematic" terminalId="connector63terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector63pad" layer="copper0"/>
     <p svgId="connector63pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector64" name="3V3">
   <description>Regulated 3.3V Output</description>
   <views>
    <breadboardView>
     <p svgId="connector64pin" layer="breadboardbreadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector64pin" layer="schematic" terminalId="connector64terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector64pad" layer="copper0"/>
     <p svgId="connector64pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
<bus id="GND">
<nodeMember connectorId="connector51"/>
<nodeMember connectorId="connector61"/>
</bus>
 </buses>
</module>
