<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.0b" moduleId="linino_dogUSB">
    <author>fabian_atlthaus</author>
    <title>linino dogUSB</title>
    <label>linino dogUSB</label>
    <date>2014-06-22</date>
    <url>http://www.linino.org/modules/linino-one/</url>
    <tags>
    <tag>linino</tag>
	<tag>usb host</tag>
    <tag>usb hub</tag>
    <tag>microcontroller</tag>
    </tags>
    <properties>
        <property name="family">Microcontroller Board (linino)</property>
        <property name="processor"></property>
        <property name="variant">linino dogUSB</property>
    </properties>
    <description>A type USB connector.
Fully compliant with USB Hub specification version 2.0 and is also backward compatible with
USB Hub specification 1.1.
Supports automatic switching between bus-power and self-power modes built-in USB 2.0 transceiver.
uSD connector with card reader.
Supports multiple sectors transfer optimize performance.
Supports port-to-slot and read/write operation.</description>
    <views>
        <iconView>
            <layers image="icon/linino_one(rev1)_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/linino_dogUSB_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/linino_dogUSB_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/linino_dogUSB_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
<connectors>
          <connector type="male" id="connector12" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12pin" layer="copper0"/>
                    <p svgId="connector12pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector13" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13pin" layer="copper0"/>
                    <p svgId="connector13pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector14" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector14pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector14pin" layer="copper0"/>
                    <p svgId="connector14pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector15" name="USB -">
            <description>USB -</description>
            <views>
                <breadboardView>
                    <p svgId="connector15pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector15pin" layer="copper0"/>
                    <p svgId="connector15pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector16" name="USB +">
            <description>USB +</description>
            <views>
                <breadboardView>
                    <p svgId="connector16pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector16pin" layer="copper0"/>
                    <p svgId="connector16pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector17" name="VDD5V">
            <description>VDD5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector17pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector17pin" layer="copper0"/>
                    <p svgId="connector17pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector18" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector18pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector18pin" layer="copper0"/>
                    <p svgId="connector18pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector19" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector19pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector19pin" layer="copper0"/>
                    <p svgId="connector19pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
          <connector type="male" id="connector23" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector23pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector23pin" layer="copper0"/>
                    <p svgId="connector23pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector24" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector24pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector24pin" layer="copper0"/>
                    <p svgId="connector24pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector25" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector25pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector25pin" layer="copper0"/>
                    <p svgId="connector25pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector26" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector26pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector26pin" layer="copper0"/>
                    <p svgId="connector26pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector27" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector27pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector27pin" layer="copper0"/>
                    <p svgId="connector27pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector28" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector28pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector28pin" layer="copper0"/>
                    <p svgId="connector28pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector29" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector29pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector29pin" layer="copper0"/>
                    <p svgId="connector29pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector30" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector30pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector30pin" layer="copper0"/>
                    <p svgId="connector30pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
       
                <connector type="male" id="connector45" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector45pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector45pin" layer="schematic" terminalId="connector45terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector45pin" layer="copper0"/>
                    <p svgId="connector45pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector46" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector46pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector46pin" layer="schematic" terminalId="connector46terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector46pin" layer="copper0"/>
                    <p svgId="connector46pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector47" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector47pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector47pin" layer="schematic" terminalId="connector47terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector47pin" layer="copper0"/>
                    <p svgId="connector47pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector48" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector48pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector48pin" layer="schematic" terminalId="connector48terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector48pin" layer="copper0"/>
                    <p svgId="connector48pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector49" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector49pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector49pin" layer="schematic" terminalId="connector49terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector49pin" layer="copper0"/>
                    <p svgId="connector49pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector50" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector50pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector50pin" layer="schematic" terminalId="connector50terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector50pin" layer="copper0"/>
                    <p svgId="connector50pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector51" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector51pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector51pin" layer="schematic" terminalId="connector51terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector51pin" layer="copper0"/>
                    <p svgId="connector51pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector52" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector52pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector52pin" layer="schematic" terminalId="connector52terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector52pin" layer="copper0"/>
                    <p svgId="connector52pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>

        </connectors>
    <buses>
        <bus>
        </bus>
   </buses>
</module>
