<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.beta.1407" moduleId="3911BBEC34">
 <version replacedby="3911BBEC34LEDModuleID">4</version>
 <author>Stefan Hermann</author>
 <title>yellow LED - 5mm</title>
 <label>LED</label>
 <date>2008-10-10</date>
 <tags>
  <tag>LED</tag>
  <tag>yellow LED</tag>
  <tag>indicator</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="package">5 mm [THT]</property>
  <property name="family">obsolete LED</property>
  <property name="color" showInLabel="yes">yellow</property>
 </properties>
 <description>A generic yellow LED (~1.8V)</description>
 <views>
  <iconView>
   <layers image="icon/LED-yellow-5mmicon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView fliphorizontal="true" flipvertical="true">
   <layers image="breadboard/LED-5mm-yellow.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/led.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/5mm_LED.svg">
    <layer layerId="copper0"/>
    <layer layerId="keepout"/>
    <layer layerId="soldermask"/>
    <layer layerId="silkscreen"/>
    <layer layerId="outline"/>
   <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="cathode" type="male">
   <description>cathode pin</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pad"/>
    <p layer="copper1" svgId="connector0pad"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="anode" type="male">
   <description>anode pin</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pad"/>
    <p layer="copper1" svgId="connector1pad"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>
