<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.18" moduleId="f9ebae12ce2b49029499a70593456637">
    <version replacedby="100milTantalumCapacitorModuleID">4</version>
    <author>Don Roberts (blog.gogozer.net)</author>
    <title>Tantalum Capacitor</title>
    <label>C</label>
    <date>2009-09-25</date>
    <tags>
        <tag>capacitor tantalum</tag>
        <tag>capacitor</tag>
        <tag>fritzing core</tag>
    </tags>
    <properties>
  <property name="family">Capacitor</property>
  <property name="Capacitance">1&#181;F</property>
  <property name="Capacitor Type">Tantalum</property>
  <property name="Rated Voltage">35V</property>
    <property name="package">THT</property></properties>
    <description>Tantalum capacitor.  Plus lead is usually marked and is usually the longer lead.</description>
    <views>
        <iconView>
            <layers image="icon/capacitor_tantalum.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/capacitor_tantalum.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/capacitor_polar.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/radial_can_200mil.svg">
                <layer layerId="copper0"/>
	      <layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="-" type="male">
            <description>negative side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="+" type="male">
            <description>positive side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>