<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.5.2b.02.18.4756" referenceFile="SPARKCORE_v1.fzp" moduleId="SPARKCORE_v10_812c474c8bfaf7c15553a915ced9e227_3">
 <version replacedby="SPARKCORE_v1_fix">5</version>
 <date>Wed Sep 3 2014</date>
 <author>Brett Walach</author>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">&#xd;
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">&#xd;
p, li { white-space: pre-wrap; }&#xd;
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:7.8pt; font-weight:400; font-style:normal;">&#xd;
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">The Spark Core is a tiny Wi-Fi development board that makes it easy to create internet-connected hardware. The Core is all you need to get started; power it over USB and in minutes you'll be controlling LEDs, switches and motors and collecting data from sensors over the internet!&lt;/p>&#xd;
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;br />&lt;/p>&#xd;
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">It has 8 digital I/O pins, 8 analog I/O pins, 8 PWM pins; UART (Serial), SPI, I2C, and JTAG peripherals available. Programmed wirelessly (through Spark Cloud), via USB or JTAG. 3.3VDC supply voltage (on board power regulator); can be powered by USB Micro 100mA typical current consumption; 300mA peak consumption (during transmit events). 2MB of external flash; EEPROM supplied by CC3000. STM32F103 microcontroller, ARM Cortex M3 architecture, 32-bit 72Mhz processor, 128KB of Flash, 20KB of RAM.&lt;/p>&lt;/body>&lt;/html></description>
 <title>Spark Core (v1.0)</title>
 <url>http://spark.io</url>
 <tags>
  <tag>Arduino Compatible</tag>
  <tag>Spark Core</tag>
  <tag>Wifi</tag>
  <tag>STM32F103</tag>
  <tag>Development Platform</tag>
  <tag>CC3000</tag>
 </tags>
 <properties>
  <property name="family">//obsolete//microcontroller board (arduino compatible)</property>
  <property name="variant">variant 2</property>
  <property name="layer"></property>
  <property name="revision">v1.0</property>
  <property name="manufacturer">Spark Labs, Inc.</property>
  <property name="part number"></property>
  <property name="name">Spark Core</property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/SPARKCORE_v10_2e5da62ec746862822eab27a1f6c2ec4_1_breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/SPARKCORE_v10_2e5da62ec746862822eab27a1f6c2ec4_1_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/SPARKCORE_v10_2e5da62ec746862822eab27a1f6c2ec4_1_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/SPARKCORE_v10_2e5da62ec746862822eab27a1f6c2ec4_1_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector id="connector41" type="male" name="A0">
   <description>Analog Input 0 / PWM1</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector41terminal" svgId="connector41pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector41pad"/>
     <p layer="copper1" svgId="connector41pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector42" type="male" name="A1">
   <description>Analog Input 1 / PWM2</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector42terminal" svgId="connector42pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector42pad"/>
     <p layer="copper1" svgId="connector42pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector43" type="male" name="A2">
   <description>Analog Input 2 / SS (SPI)</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector43terminal" svgId="connector43pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector43pad"/>
     <p layer="copper1" svgId="connector43pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector44" type="male" name="A3">
   <description>Analog Input 3 / SCK (SPI)</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector44terminal" svgId="connector44pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector44pad"/>
     <p layer="copper1" svgId="connector44pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector45" type="male" name="A4">
   <description>Analog Input 4 / PWM3 / MISO (SPI)</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector45terminal" svgId="connector45pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector45pad"/>
     <p layer="copper1" svgId="connector45pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector46" type="male" name="A5">
   <description>Analog Input 5 / PWM4 / MOSI (SPI)</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector46terminal" svgId="connector46pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector46pad"/>
     <p layer="copper1" svgId="connector46pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector47" type="male" name="A6">
   <description>Analog Input 6 / PWM5</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector47terminal" svgId="connector47pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector47pad"/>
     <p layer="copper1" svgId="connector47pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector48" type="male" name="A7">
   <description>Analog Input 7 / PWM6</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector48terminal" svgId="connector48pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector48pad"/>
     <p layer="copper1" svgId="connector48pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector49" type="male" name="TX">
   <description>Serial1 UART Transmit</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector49terminal" svgId="connector49pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector49pad"/>
     <p layer="copper1" svgId="connector49pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector50" type="male" name="RX">
   <description>Serial1 UART Receive</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector50terminal" svgId="connector50pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector50pad"/>
     <p layer="copper1" svgId="connector50pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector51" type="male" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector51terminal" svgId="connector51pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector51pad"/>
     <p layer="copper1" svgId="connector51pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector52" type="male" name="VIN">
   <description>Diode drop below USB V+ / Input to 3.3V Regulator (3.6 - 6V max input)</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector52terminal" svgId="connector52pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector52pad"/>
     <p layer="copper1" svgId="connector52pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector53" type="male" name="D0">
   <description>Digital Input/Output 0 / SDA (ISC) / PWM7</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector53terminal" svgId="connector53pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector53pad"/>
     <p layer="copper1" svgId="connector53pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector54" type="male" name="D1">
   <description>Digital Input/Output 1 / SCL (I2C) / PWM8</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector54pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector54terminal" svgId="connector54pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector54pad"/>
     <p layer="copper1" svgId="connector54pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector55" type="male" name="D2">
   <description>Digital Input/Output 2</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector55terminal" svgId="connector55pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector55pad"/>
     <p layer="copper1" svgId="connector55pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector56" type="male" name="D3">
   <description>Digital Input/Output 3</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector56terminal" svgId="connector56pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector56pad"/>
     <p layer="copper1" svgId="connector56pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector57" type="male" name="D4">
   <description>Digital Input/Output 4</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector57terminal" svgId="connector57pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector57pad"/>
     <p layer="copper1" svgId="connector57pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector58" type="male" name="D5">
   <description>Digital Input/Output 5</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector58terminal" svgId="connector58pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector58pad"/>
     <p layer="copper1" svgId="connector58pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector59" type="male" name="D6">
   <description>Digital Input/Output 6</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector59terminal" svgId="connector59pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector59pad"/>
     <p layer="copper1" svgId="connector59pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector60" type="male" name="D7">
   <description>Digital Input/Output 7</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector60terminal" svgId="connector60pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector60pad"/>
     <p layer="copper1" svgId="connector60pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector61" type="male" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector61terminal" svgId="connector61pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector61pad"/>
     <p layer="copper1" svgId="connector61pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector62" type="male" name="3V3*">
   <description>Filtered 3.3V Output (Aref input)</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector62terminal" svgId="connector62pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector62pad"/>
     <p layer="copper1" svgId="connector62pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector63" type="male" name="RST">
   <description>Reset Input (Active Low)</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector63pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector63terminal" svgId="connector63pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector63pad"/>
     <p layer="copper1" svgId="connector63pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector64" type="male" name="3V3">
   <description>Regulated 3.3V Output</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector64pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector64terminal" svgId="connector64pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector64pad"/>
     <p layer="copper1" svgId="connector64pad"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="GND">
   <nodeMember connectorId="connector51"/>
   <nodeMember connectorId="connector61"/>
  </bus>
 </buses>
</module>
